{"text_format":"1","workbook":"xlsx","n_sheets":14,"sheets":["Cover","Sheet1","Details & Checklist","Product_Part_1","BarrierTesting","TerminalCrashCushionTest","Non-RedirectiveCrashCushionTest","Product_Part_2","TCDTest","TMAs","RearUnderrunDevicesTest","Bollards","SupportStructuresPolesTest","Additional Information"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":32,"n_cols":4,"rows_kept":32,"cut":false,"hidden":false,"merged":[[10,1,10,3],[15,1,15,3],[12,1,13,1],[0,1,0,3],[1,1,8,3],[31,2,31,3],[30,2,30,3],[12,3,13,3],[29,1,29,3],[27,1,27,3]]}
[null,"Austroads Safety Barrier Assessment Panel\nSUBMISSION TEMPLATE"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Please select the relevant AS/NZS Standard 3845 - Part 1 or Part 2.  Once you make the relevant selection the required sheets will be available for completion"]
[]
[null,"AS/NZS 3845 - Part 1 Products",null,"AS/NZS 3845 - Part 2 Products"]
[]
[]
[null,"Please select the product type relevant to your submission. Only one product permitted per submission template.\nOnce you make the relevant selection the relevant sheets will be available for completion."]
[]
[null,"Longitudinal Barrier\nBarriers must include connection to terminals or crash cushions\n",null,"Traffic Control Devices & LCDs"]
[]
[null,"Terminals or Redirective Crash Cushions",null,"Truck or Trailers Mounted Attenuators"]
[]
[null,"Non-directive Crash Cushions",null,"Rear Underrun Devices"]
[]
[null,null,null,"Bollards             "]
[]
[null,null,null,"Support Structure and Poles"]
[]
[null,"Please submit the completed electronic workbook to the ASBAP Secretariat along with the supporting information in electronic form.  No hardcopy information accepted.  \nYou may also submit a PDF copy for records purpose only (if desired)."]
[]
[null,"Version Control"]
[null,"Version","Date"]
[null,2,"April 2018"]

{"sheet":"Sheet1","index":1,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["MASH"]
["EN1317"]
["NCHRP 350"]

{"sheet":"Details & Checklist","index":2,"n_rows":67,"n_cols":5,"rows_kept":67,"cut":false,"hidden":false,"merged":[[53,1,53,2],[48,1,48,2],[0,1,0,2],[3,1,3,2],[10,1,10,2],[17,1,17,2],[24,1,24,2],[31,1,31,2],[38,1,38,2],[43,1,43,2],[1,1,1,2],[46,1,46,2]]}
[null,"Details"]
[null,"Please be advised that the row heights will increase automatically as information is provided"]
[]
[null,"Proponent Details"]
[null,"Name: "]
[null,"Primary Contact:"]
[null,"Address:"]
[null,"Phone:"]
[null,"Email:"]
[]
[null,"System Owner"]
[null,"Name: "]
[null,"Primary Contact:"]
[null,"Address:"]
[null,"Phone:"]
[null," Email:"]
[]
[null,"System Manufacturer"]
[null,"Name: "]
[null,"Primary Contact:"]
[null,"Address:"]
[null,"Phone:"]
[null," Email:"]
[]
[null,"Distributor Details - Australia"]
[null,"Name: "]
[null,"Primary Contact:"]
[null,"Address:"]
[null,"Phone:"]
[null," Email:"]
[]
[null,"Distributor Details - New Zealand"]
[null,"Name: "]
[null,"Primary Contact:"]
[null,"Address:"]
[null,"Phone:"]
[null," Email:"]
[]
[null,"Product"]
[null,"Product Type:"]
[null,"Product Name:"]
[null,"Variant:"]
[]
[null,"Submission"]
[null,"Submission Date:"]
[]
[null,"By submitting a product for assessment the Proponent certifies that they have the legal right and authority to provide\nthe information and agrees that all information may be used by road agencies for their business activities and that \nthe product complies with all requirements covered by AS/NZS 3845 Part 1 or Part 2"]
[]
[null,"Austroads Safety Barrier Assessment Panel Secretariat Use Only"]
[null,"Date Submission Received:"]
[null,"Date Submission Checked:"]
[null,"ASBAP Meeting Date:              "]
[]
[null,"Submission Checklist"]
[null,"Complete checklist of attachments below before submitting product.",null,null,"ASBAP Secretariat Use Only"]
[null,"Item",null,"ü","ü"]
[null,1,"Cover letter",false,false]
[null,2,"Submission template (this document)",null,false]
[null,3,"Product Manual(s)"]
[null,4,"Training documentation"]
[null,5,"Product drawings (.JPG or PDF format)"]
[null,6,"Product photos (.JPG format)"]
[null,7,"Materials and Specifications"]
[null,8,"Crash test videos (.AVI format0"]
[null,9,"Crash test reports"]
[null,10,"Crash test photos (.JPG format)",null,true]
[null,11,"Barrier/Terminal/Crash Cushion/Gate Proponent Letters and Interface Diagrams"]

{"sheet":"Product_Part_1","index":3,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":true,"merged":[[12,3,12,4],[13,3,13,4],[14,3,14,4],[15,1,15,5],[0,1,0,5],[4,3,4,4],[5,3,5,4],[6,3,6,4],[7,3,7,4],[1,1,1,5],[4,1,4,2],[3,1,3,5],[8,3,8,4],[9,3,9,4],[10,3,10,4],[11,3,11,4]]}
[null,"Product Details and Conditions – AS/NZS 3845 – Part 1 Products "]
[null,"Please be advised that the row height will increase automatically as information is provided"]
[null,"Complete ‘all relevant’ fields in the tables below:"]
[null,"Safety Barriers, Terminals, Crash Cushions, Barrier Gates"]
[null,"Product",null,"Details",null,"AS/NZS"]
[null,"Product Name ",null,null,null,"N/A"]
[null,"Classification","(safety barrier, terminal, crash cushion, gate)",null,null,"N/A"]
[null,"Use","(temporary/permanent)",null,null,"N/A"]
[null,"Product Description \n","(describe how the product is designed to operate e.g. Gating/non-gating, re-directive, capture etc)",null,null,"N/A"]
[null,"Type"," (wire rope, concrete, plastic water filled, etc)",null,null,"N/A"]
[null,"Changes to Existing Product",null,null,null,"N/A"]
[null,null,"Variant",null,null,"N/A"]
[null,null,"Modified Configuration",null,null,"N/A"]
[null,null,"Additional Component",null,null,"N/A"]
[null,"Product Manual ","Must include date and/or version number",null,null,"Clause 2.2"]
[]
[null,"Terminals and Connections"]
[null,"Public/Proprietary Products","Name","Details","Proponent Justification","AS/NZS"]
[null,null,"W-Beam Guardrail",null,null,"Clause 2.4"]
[null,"Public Domain Products","Thrie Beam Guardrail",null,null,"Clause 2.4"]
[null,null,"Type F Concrete",null,null,"Clause 2.4"]
[null,null,null,null,null,"Clause 2.4"]
[null,null,null,null,null,"Clause 2.4"]
[null,"Proprietary Products",null,null,null,"Clause 2.4"]
[null,null,null,null,null,"Clause 2.4"]
[null,null,null,null,null,"Clause 2.4"]
[null,null,null,null,null,"Clause 2.4"]
[]
[null,"Design",null,"Details","Proponent Justification","AS/NZS"]
[null,"Slope limit ","(horizontal to vertical -%)",null,null,"N/A"]
[null,"System width ","(metres)",null,null,"N/A"]
[null,"Minimum distance to excavation ","(metres)",null,null,"N/A"]
[null,"Minimum median width","(metres)",null,null,"N/A"]
[null,"Use",null,"(permitted, not permitted or comment)",null,"Clause 2.3 & 2.5"]
[null,null,"Gore area",null,null,"Clause 2.3 & 2.5"]
[null,null,"Pedestrian area"]
[null,null,"Cycleway",null,null,"Clause 2.3 & 2.5"]
[null,null,"Frequent impact likely",null,null,"Clause 2.3 & 2.5"]
[null,null,"Remote location",null,null,"Clause 2.3 & 2.5"]
[null,null,"Median",null,null,"Clause 2.3 & 2.5"]

{"sheet":"BarrierTesting","index":4,"n_rows":49,"n_cols":9,"rows_kept":49,"cut":false,"hidden":true,"merged":[[0,0,0,7],[29,0,29,2],[40,0,40,13],[41,0,41,7],[32,6,33,6],[32,7,33,7],[32,0,33,0],[1,0,1,7],[3,0,3,8]]}
["Crash Testing – AS/NZS 3845 – Part 1 Products"]
["Please be advised that the row height will increase as information is provided"]
[]
["Longitudinal Safety Barriers"]
["Test Level","Crash Test Standard","MASH\nTest No","Equivalent Test No","Undertaken\n(ü or x)","Crash Test Report No","AS/NZS 3845.1\nClause","Proponent justification required for tests that have not been undertaken","MASH equivalence rating and justification\n(for testing guidelines other than MASH)"]
[null,null,"Test 1-10"]
["Test Level 1",null,"Test 1-11",null,null,null,"Clause 4.3"]
[null,null,"Test 1-20*"]
[null,null,"Test 1-21"]
[null,null,"Test 2-10"]
["Test Level 2",null,"Test 2-11",null,null,null,"Clause 4.3"]
[null,null,"Test 2-20*"]
[null,null,"Test 2-21"]
[null,null,"Test 3-10"]
["Test Level 3",null,"Test 3-11",null,null,null,"Clause 4.3"]
[null,null,"Test 3-20*"]
[null,null,"Test 3-21"]
[null,null,"Test 4-10"]
[null,null,"Test 4-11"]
["Test Level 4",null,"Test 4-12",null,null,null,"Clause 4.3"]
[null,null,"Test 4-20*"]
[null,null,"Test 4-21"]
[null,null,"Test 4-22"]
[null,null,"Test 5-10"]
[null,null,"Test 5-11"]
["Test Level 5",null,"Test 5-12",null,null,null,"Clause 4.3"]
[null,null,"Test 5-20*"]
[null,null,"Test 5-21"]
[null,null,"Test 5-22"]
["* Test is optional"]
[]
["Tested Containment "]
["Tested Containment Level\n","Point of redirection/\nneed (m)","Minimum length of barrier","Post/pin spacing ","Dynamic deflection","Working width","AS/NZS 3845.1\nClause","Proponent Justification"]
[null,"Leading & Trailing","(m)","(m)","(m)","(m)"]
[]
[]
[null,null,null,null,null,null,"Clause 2.3"]
[]
[]
[]
[]
["Foundation Pavement Conditions"]
["Pavement","Use\n(Permitted/Not Permitted)","Accepted Speed (max)","Pavement Construction","Post/Pin Spacing (m)","Post/Pin Type","AS/NZS","Proponent Justification (Test Number)"]
["Concrete"]
["Deep lift asphaltic concrete",null,null,null,null,null,"Clause 2.3"]
["Asphaltic concrete over granular",null,null,null,null,null,"and"]
["Flush seal over granular",null,null,null,null,null,"Clause 2.5"]
["Unsealed compacted formation"]
["Natural surface"]

{"sheet":"TerminalCrashCushionTest","index":5,"n_rows":51,"n_cols":9,"rows_kept":51,"cut":false,"hidden":true,"merged":[[3,0,3,8],[0,0,0,8],[1,0,1,8],[42,0,42,13],[43,0,43,7],[31,0,31,2],[33,0,33,7],[34,0,35,0],[34,6,35,6],[34,7,35,7]]}
["Crash Testing – AS/NZS 3845 – Part 1 Products"]
["Please be advised that row heights will increase as information is provided"]
[]
["Terminals and Redirective Crash Cushions"]
["Test Level","Crash Test Standard","MASH\nTest No","Equivalent Test No","Undertaken\n(ü or x)","Crash Test Report No","AS/NZS 3845.1\nClause","Proponent justification required for tests that have not been undertaken","MASH equivalence rating and justification\n(for testing guidelines other than MASH)"]
[null,null,"Test 1-30"]
[null,null,"Test 1-31"]
[null,null,"Test 1-32"]
["Test Level 1",null,"Test 1-33",null,null,null,"Clause 4.3"]
[null,null,"Test 1-34"]
[null,null,"Test 1-35"]
[null,null,"Test 1-36"]
[null,null,"Test 1-37"]
[null,null,"Test 2-30"]
[null,null,"Test 2-31"]
[null,null,"Test 2-32"]
[null,null,"Test 2-33"]
["Test Level 2",null,"Test 2-34",null,null,null,"Clause 4.3"]
[null,null,"Test 2-35"]
[null,null,"Test 2-36"]
[null,null,"Test 2-37"]
[null,null,"Test 2-38"]
[null,null,"Test 3-30"]
[null,null,"Test 3-31"]
[null,null,"Test 3-32"]
["Test Level 3",null,"Test 3-33",null,null,null,"Clause 4.3"]
[null,null,"Test 3-34"]
[null,null,"Test 3-35"]
[null,null,"Test 3-36"]
[null,null,"Test 3-37"]
[null,null,"Test 3-38"]
[]
[]
["Tested Containment "]
["Tested Containment Level\n","Point of redirection/\nneed (m)","Post/pin spacing ","Dynamic deflection","Working width",null,"AS/NZS 3845.1\nClause","Proponent Justification"]
[null,"Leading & Trailing","(m)","(m)","(m)"]
[]
[]
[null,null,null,null,null,null,"Clause 2.3"]
[]
[]
[]
[]
["Foundation Pavement Conditions"]
["Pavement","Use\n(Permitted/Not Permitted)","Accepted Speed (max)","Pavement Construction","Post/Pin Spacing\n(m)","Post/Pin Type","AS/NZS","Proponent Justification (Test Number)"]
["Concrete"]
["Deep lift asphaltic concrete",null,null,null,null,null,"Clause 2.3"]
["Asphaltic concrete over granular",null,null,null,null,null,"and"]
["Flush seal over granular",null,null,null,null,null,"Clause 2.5"]
["Unsealed compacted formation"]
["Natural surface"]

{"sheet":"Non-RedirectiveCrashCushionTest","index":6,"n_rows":43,"n_cols":9,"rows_kept":43,"cut":false,"hidden":true,"merged":[[1,0,1,8],[3,0,3,8],[0,0,0,8],[34,0,34,13],[35,0,35,7],[23,0,23,2],[25,0,25,7],[26,0,27,0],[26,6,27,6],[26,7,27,7],[26,4,27,4]]}
["Crash Testing – AS/NZS 3845 – Part 1 Products"]
["Please be advised that row heights will increase as information is provided"]
[]
["Non-redirective Crash Cushions"]
["Test Level","Crash Test Standard","MASH\nTest No","Equivalent Test No","Undertaken\n(ü or x)","Crash Test Report No","AS/NZS 3845.1\nClause","Proponent justification required for tests that have not been undertaken","MASH equivalence rating and justification\n(for testing guidelines other than MASH)"]
[null,null,"Test 1-40"]
[null,null,"Test 1-41"]
["Test Level 1",null,"Test 1-42",null,null,null,"Clause 4.3"]
[null,null,"Test 1-43"]
[null,null,"Test 1-44"]
[null,null,"Test 1-45"]
[null,null,"Test 2-40"]
[null,null,"Test 2-41"]
["Test Level 2",null,"Test 2-42",null,null,null,"Clause 4.3"]
[null,null,"Test 2-43"]
[null,null,"Test 2-44"]
[null,null,"Test 2-45"]
[null,null,"Test 3-40"]
[null,null,"Test 3-41"]
["Test Level 3",null,"Test 3-42",null,null,null,"Clause 4.3"]
[null,null,"Test 3-43"]
[null,null,"Test 3-44"]
[null,null,"Test 3-45"]
[]
[]
["Tested Containment "]
["Tested Containment Level\n","Post/pin spacing ","Dynamic deflection","Working width",null,null,"AS/NZS 3845.1\nClause","Proponent Justification"]
[null,"(m)","(m)","(m)"]
[]
[]
[null,null,null,null,null,null,"Clause 2.3"]
[]
[]
[]
[]
["Foundation Pavement Conditions"]
["Pavement","Use\n(Permitted/Not Permitted)","Accepted Speed (max)","Pavement Construction","Post/Pin Spacing (m)","Post/Pin Type","AS/NZS","Proponent Justification (Test Number)"]
["Concrete"]
["Deep lift asphaltic concrete",null,null,null,null,null,"Clause 2.3"]
["Asphaltic concrete over granular",null,null,null,null,null,"and"]
["Flush seal over granular",null,null,null,null,null,"Clause 2.5"]
["Unsealed compacted formation"]
["Natural surface"]

{"sheet":"Product_Part_2","index":7,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":true,"merged":[[6,3,6,4],[38,1,38,5],[12,3,12,4],[13,3,13,4],[14,1,14,5],[15,1,15,2],[28,1,28,2],[29,1,29,5],[7,3,7,4],[8,3,8,4],[9,3,9,4],[10,3,10,4],[11,3,11,4],[0,1,0,5],[1,1,1,5],[3,1,3,5],[4,3,4,4],[5,3,5,4],[4,1,4,2]]}
[null,"Product Details and Conditions – AS/NZS 3845 – Part 2 Products "]
[null,"Please be advised that the row height will increase automatically as information is provided"]
[null,"Complete ‘all relevant’ fields in the tables below:"]
[null,"Bollards, Longitudinal Channelizing Devices, Truck or Trailer Mounted Attenuators, Rear Underrun Protection Devices, Sign Support Structure and Poles"]
[null,"Product",null,"Details",null,"AS/NZS"]
[null,"Product Name ",null,null,null,"N/A"]
[null,"Classification","(Bollards, Longitudinal Channelizing Devices, Truck or Trailer Mounted Attenuators, Rear Underrun Protection Devices, Sign Support Structure and Poles)",null,null,"N/A"]
[null,"Use","(temporary/permanent)",null,null,"N/A"]
[null,"Product Description \n","(describe how the product is designed to operate e.g. interconnected LCD, Non-interconnected LCD, Break Away, Energy Absorbing, etc)",null,null,"N/A"]
[null,"Changes to Existing Product",null,null,null,"N/A"]
[null,null,"Variant",null,null,"N/A"]
[null,null,"Modified Configuration",null,null,"N/A"]
[null,null,"Additional Component",null,null,"N/A"]
[null,"Product Manual ","Must include date and/or version number",null,null,"Clause 2.2"]
[]
[null,"Design",null,"Details","Proponent Justification","AS/NZS"]
[null,"Slope limit ","(horizontal to vertical -%)",null,null,"N/A"]
[null,"System width ","(metres)",null,null,"N/A"]
[null,"Minimum distance to excavation ","(metres)",null,null,"N/A"]
[null,"Minimum median width","(metres)",null,null,"N/A"]
[null,null,null,"(permitted, not permitted or comment)",null,"Clause 2.3 & 2.5"]
[null,null,"Gore area",null,null,"Clause 2.3 & 2.5"]
[null,"Use","Pedestrian area"]
[null,null,"Cycleway",null,null,"Clause 2.3 & 2.5"]
[null,null,"Frequent impact likely",null,null,"Clause 2.3 & 2.5"]
[null,null,"Remote location",null,null,"Clause 2.3 & 2.5"]
[null,null,"Median",null,null,"Clause 2.3 & 2.5"]
[]
[null,"Design",null,"Details","Proponent Justification","AS/NZS"]
[null,"Truck Mounted Attenuators and Rear Underrun Protection Devices"]
[null,"Make, model, ballasting","Tested Truck",null,null,"Clause 6.4 & 7.4"]
[null,"Truck masses and dimensions","(that RUPD and TMAs can be attached to)",null,null,"Clause 6.4 & 7.4"]
[null,"Truck braking during operation","(metres)",null,null,"Clause 6.4 & 7.4"]
[null,"Length, width, height of RUPD",null,null,null,"Clause 6.4 & 7.4"]
[null,"Height of TMA ","(with respect to ground)",null,null,"Clause 6.4 & 7.4"]
[null,"Length of supporting truck",null,null,null,"Clause 6.4 & 7.4"]
[null,"Mass of RUPD/TMA","(include supporting hardware)",null,null,"Clause 6.4 & 7.4"]
[null,"Condition & type of brakes/blocks","(used to reduce or prevent vehicle roll ahead)",null,null,"Clause 6.4 & 7.4"]
[null,"Energy Absorbing Sign Support Structures and Poles"]
[null,"Structural calculations",null,null,null,"Clause 9.4"]
[null,"Support configurations",null,null,null,"Clause 9.4"]

{"sheet":"TCDTest","index":8,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":true,"merged":[[0,0,0,8],[1,0,1,8],[3,0,3,8],[14,0,14,8],[24,1,24,2],[32,0,32,13],[33,0,33,7],[21,0,21,2],[23,0,23,7],[24,0,25,0],[24,6,25,6],[24,7,25,7]]}
["Crash Testing – AS/NZS 3845 – Part 2 Products"]
["Please be advised that row heights will increase as information is provided"]
[]
["Workzone Traffic Control Devices & Longitudinal Channelizing Devices (Non-interconnected)"]
["Test Level","Crash Test Standard","MASH\nTest No","Equivalent Test No","Undertaken\n(ü or x)","Crash Test Report No","AS/NZS 3845.2\nClause","Proponent justification required for tests that have not been undertaken","MASH equivalence rating and justification\n(for testing guidelines other than MASH)"]
[null,null,"Test 1-70"]
["Test Level 1",null,"Test 1-71",null,null,null,"Clause 5.3"]
[null,null,"Test 1-72"]
[null,null,"Test 2-70"]
["Test Level 2",null,"Test 2-71",null,null,null,"Clause 5.3"]
[null,null,"Test 2-72"]
[null,null,"Test 3-70"]
["Test Level 3",null,"Test 3-71",null,null,null,"Clause 5.3"]
[null,null,"Test 3-72"]
["Longitudinal Channelizing Devices (Interconnected)"]
["Test Level 1",null,"Test 1-90",null,null,null,"Clause 5.3"]
[null,null,"Test 1-91"]
["Test Level 2",null,"Test 2-90",null,null,null,"Clause 5.3"]
[null,null,"Test 2-91"]
["Test Level 3",null,"Test 3-90",null,null,null,"Clause 5.3"]
[null,null,"Test 3-91"]
[]
[]
["Tested Containment "]
["Tested Containment Level\n","Point of redirection/point of need\n(m)",null,"Minimum length of barrier","Dynamic deflection","Working width","AS/NZS 3845.2\nClause","Proponent Justification"]
[null,"Leading","Trailing","(m)","(m)","(m)"]
[]
[]
[null,null,null,null,null,null,"Clause 2.3"]
[]
[]
[]
[]
["Foundation Pavement Conditions"]
["Pavement","Use\n(Permitted/Not Permitted)","Accepted Speed (max)","Pavement Construction",null,"`","AS/NZS","Proponent Justification (Test Number)"]
["Concrete"]
["Deep lift asphaltic concrete"]
["Asphaltic concrete over granular",null,null,null,null,null,"Clause 2.3"]
["Flush seal over granular"]
["Unsealed compacted formation"]
["Natural surface"]

{"sheet":"TMAs","index":9,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":true,"merged":[[22,0,22,2],[20,0,20,2],[3,0,3,8],[1,0,1,8],[0,0,0,8]]}
["Crash Testing – AS/NZS 3845 – Part 2 Products"]
["Please be advised that row heights will increase as information is provided"]
[]
["Truck or Trailer Mounted Attenuators"]
["Test Level","Crash Test Standard","MASH\nTest No","Equivalent Test No","Undertaken\n(ü or x)","Crash Test Report No","AS/NZS 3845.2\nClause","Proponent justification required for tests that have not been undertaken","MASH equivalence rating and justification\n(for testing guidelines other than MASH)"]
[null,null,"Test 1-50"]
[null,null,"Test 1-51"]
["Test Level 1",null,"Test 1-52",null,null,null,"Clause 6.3"]
[null,null,"Test 1-53"]
[null,null,"Test 1-54*"]
[null,null,"Test 2-50"]
[null,null,"Test 2-51"]
["Test Level 2",null,"Test 2-52",null,null,null,"Clause 6.3"]
[null,null,"Test 2-53"]
[null,null,"Test 2-54*"]
[null,null,"Test 3-50"]
[null,null,"Test 3-51"]
["Test Level 3",null,"Test 3-52",null,null,null,"Clause 6.3"]
[null,null,"Test 3-53"]
[null,null,"Test 3-54*"]
["* Test is optional"]
[]
["Tested Containment "]
["Tested Containment Level\n","Support Truck Roll Ahead Distance","AS/NZS 3845.2\nClause"]
[]
[]
[null,null,"Clause 2.3"]

{"sheet":"RearUnderrunDevicesTest","index":10,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":true,"merged":[[0,0,0,8],[22,5,23,5],[22,6,23,6],[22,7,23,7],[1,0,1,8],[15,0,15,1],[16,6,17,6],[16,7,17,7],[13,0,13,2],[16,0,17,0],[16,1,17,1],[16,5,17,5],[3,0,3,8],[15,5,15,7]]}
["Crash Testing – AS/NZS 3845 – Part 2 Products"]
["Please be advised that row heights will increase as information is provided"]
[]
["Rear Underrun Protection Devices"]
["Test Level","Crash Test Standard","MASH\nTest No","Equivalent Test No","Undertaken\n(ü or x)","Crash Test Report No","AS/NZS 3845.2\nClause","Proponent justification required for tests that have not been undertaken","MASH equivalence rating and justification\n(for testing guidelines other than MASH)"]
[null,null,"Test 1-51"]
["Test Level 1",null,"Test 1-52",null,null,null,"Clause 7.3"]
[null,null,"Test 1-54"]
[null,null,"Test 1-55"]
[null,null,"Test 2-51"]
["Test Level 2",null,"Test 2-52",null,null,null,"Clause 7.3"]
[null,null,"Test 2-54"]
[null,null,"Test 2-55"]
[]
[]
["Tested Containment ",null,null,null,null,"Barrier Connections"]
["Tested Containment Level\n","AS/NZS 3845.2\nClause",null,null,null,"Public Domain Products","Details","Proponent Justification"]
[]
[null,null,null,null,null,"W-beam guardrail"]
[null,null,null,null,null,"Thrie-beam guardrail"]
[null,"Clause 2.3",null,null,null,"Type F concrete"]
[]
[null,null,null,null,null,"Public Domain Products","Details","Proponent Justification"]

{"sheet":"Bollards","index":11,"n_rows":34,"n_cols":9,"rows_kept":34,"cut":false,"hidden":true,"merged":[[3,0,3,8],[1,0,1,8],[0,0,0,8],[26,0,26,7],[17,1,18,1],[17,2,18,2],[16,0,16,2],[14,0,14,2],[17,0,18,0],[25,0,25,13]]}
["Crash Testing – AS/NZS 3845 – Part 2 Products"]
["Please be advised that row heights will increase as information is provided"]
[]
["Bollards"]
["Test Level","Crash Test Standard","MASH\nTest No","Equivalent Test No","Undertaken\n(ü or x)","Crash Test Report No","AS/NZS 3845.2\nClause","Proponent justification required for tests that have not been undertaken","MASH equivalence rating and justification\n(for testing guidelines other than MASH)"]
[null,null,"Test 1-100"]
["Test Level 1",null,"Test 1-101",null,null,null,"Clause 8.5"]
[null,null,"Test 1-102"]
[null,null,"Test 2-100"]
["Test Level 2",null,"Test 2-101",null,null,null,"Clause 8.5"]
[null,null,"Test 2-102"]
[null,null,"Test 3-100"]
["Test Level 3",null,"Test 3-101",null,null,null,"Clause 8.5"]
[null,null,"Test 3-102"]
["Refer to AS/NZS 3845 for test details"]
[]
["Tested Containment "]
["Tested Containment Level","Vehicle Intrusion","Post Impact Trajectory & Breakaway Parts"]
[]
[]
[]
[]
[]
[]
[]
[]
["Foundation Pavement Conditions"]
["Pavement","Use\n(Permitted/Not Permitted)","Accepted Speed (max)","Pavement \nConstruction",null,null,"AS/NZS 3845.2 Clause","Proponent Justification (Test Number)"]
["Concrete"]
["Deep lift asphaltic concrete"]
["Asphaltic concrete over granular",null,null,null,null,null,"Clause 2.3"]
["Flush seal over granular"]
["Unsealed compacted formation"]
["Natural surface"]

{"sheet":"SupportStructuresPolesTest","index":12,"n_rows":50,"n_cols":9,"rows_kept":50,"cut":false,"hidden":true,"merged":[[42,0,42,7],[33,0,33,2],[31,0,31,2],[1,0,1,8],[0,0,0,8],[3,0,3,8],[11,0,11,8],[21,0,21,8],[41,0,41,13]]}
["Crash Testing – AS/NZS 3845 – Part 2 Products"]
["Please be advised that row heights will increase as information is provided"]
[]
["Support Structure and Poles (Energy Absorbing)"]
["Test Level","Crash Test Standard","MASH\nTest No","Equivalent Test No","Undertaken\n(ü or x)","Crash Test Report No","AS/NZS 3845.2\nClause","Proponent justification required for tests that have not been undertaken","MASH equivalence rating and justification\n(for testing guidelines other than MASH)"]
["Test Level 1",null,"Test 1-40",null,null,null,"Clause 9.3"]
[null,null,"Test 1-41"]
["Test Level 2",null,"Test 2-40",null,null,null,"Clause 9.3"]
[null,null,"Test 2-41"]
["Test Level 3",null,"Test 3-40",null,null,null,"Clause 9.3"]
[null,null,"Test 3-41"]
["Support Structure and Poles (Breakaway Sign Support Structures or Poles)"]
[null,null,"Test 1-60"]
["Test Level 1",null,"Test 1-61",null,null,null,"Clause 9.3"]
[null,null,"Test 1-62"]
[null,null,"Test 2-60"]
["Test Level 2",null,"Test 2-61",null,null,null,"Clause 9.3"]
[null,null,"Test 2-62"]
[null,null,"Test 3-60"]
["Test Level 3",null,"Test 3-61",null,null,null,"Clause 9.3"]
[null,null,"Test 3-62"]
["Support Structure and Poles (Break away Utility/Lighting Poles)"]
[null,null,"Test 1-80"]
["Test Level 1",null,"Test 1-81",null,null,null,"Clause 9.3"]
[null,null,"Test 1-82"]
[null,null,"Test 2-80"]
["Test Level 2",null,"Test 2-81",null,null,null,"Clause 9.3"]
[null,null,"Test 2-82"]
[null,null,"Test 3-80"]
["Test Level 3",null,"Test 3-81",null,null,null,"Clause 9.3"]
[null,null,"Test 3-82"]
[]
[]
["Tested Containment "]
["Tested Containment Level\n","Post Impact Trajectory & Breakaway Parts","AS/NZS 3845.2\nClause"]
[]
[]
[null,null,"Clause 2.3 & 9.4"]
[]
[]
[]
[]
["Foundation Pavement Conditions"]
["Pavement","Use\n(Permitted/Not Permitted)","Accepted Speed (max)","Pavement \nConstruction",null,null,"AS/NZS 3845.2 Clause","Proponent Justification (Test Number)"]
["Concrete"]
["Deep lift asphaltic concrete"]
["Asphaltic concrete over granular",null,null,null,null,null,"Clause 2.3"]
["Flush seal over granular"]
["Unsealed compacted formation"]
["Natural surface"]

{"sheet":"Additional Information","index":13,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[null,"Additional Information"]
[null,"Please be advised that the row height will increase automatically as information is provided"]